Before you begin to install any accessories. Make sure to check with a certified Victory mechanic. 
Note for all Bolts used on this application Loctite Is needed. 
Mount Spacers provided in Holes inside Factory Fender rail You have removed from your Victory Motorcycle. See picture Below; 

Use Bolts and washers provided and insert through Backrest Mounting rail with washers on the outside.  The bolts will also go through sapcers and follow through the factory fender rail See picture Below; 

Install each side Into Fender and thread into Motorcycle subframe as fender rail was installed before removing the fender Rails. Its Important to not tighten at this point or wil not be ble to install the backrest pad. See picture Below; 
.
Install backrest Pad to the Mounting bar using 2 bolts provided. If already assembled before shipping please remove and apply loctite and verify tightness. See picture Below; 

Picture Below is the mounting spacer. Note the rounded side will be installed to the rounded mounting bar. See picture Below; 

Using the bolts and washers provided install mounting bar to the Side Rails. The bolts will install through the mounting rail, through the spacer then thread into the Mounting bar See picture Below; 

Below is ho your backrest should look installed. Tighten the upper bolts to the Mounting bar with pad first. Nest Tighten the 4 Bolts holding the side reails and fender rails on. 

Thank You for Purchasing a Victory Only Product. 
www.VictoryOnly.com